PING (Packet Internet Groper) command is used to check the network connectivity between host and server/host. This command takes as input the IP address or the URL and sends a data packet to the specified address with the message “PING” and get a response from the server/host this time is recorded which is called latency.

**Finger** may be used to look up users on a remote machine. The format is to specify a user as "user@host", or "@host", where the default output format for the former is the -l style, and the default output format for the latter is the -s style. The -l option is the only option that may be passed to a remote machine

**arp command** manipulates the System’s ARP cache. It also allows a complete dump of the ARP cache. ARP stands for Address Resolution Protocol.

Diskperf is a Microsoft Windows command for starting and stopping disk performance counters for Performance Monitor (System Monitor in Windows 2000)

To simply use the **rcp** command, just provide the source and destination to rcp command with a colon used to separate the host and the data.